Palm'n'Stein 

To install, use the Palm Desktop to install the following files
from the CD-ROM:

PNStein.prc
Reg.pdb

In addition, 2g owners should install the DTC library found in
the file Dtc.pdb

To run the logger:

1) Take the guided tour: 

http://206.124.12.138/codsm/tunerstein/webpage/4.1/palm%27n%27stein.html

2) Choose Palm'n'Stein from the menu

3) At this point, make sure you have taken the guided tour!

4) Connect the Palm to the logger cable/interface, and then 
plug the adapter into the interface under the dash.

5) Start the car.

6) Press "F1".  In a few seconds, logging will begin.  If the Palm
is not connected properly, you will get an error message.  Resolve
the problem and press "F1" again.

During logging, you may press pause.  No items will be written to the 
log file while you are "paused", and charting will stop.  To resume
logging, press "F1" again.

Press "Stop" when you are done logging.  You can then save or discard
the file.

7) To play back, press f4.  Select a log file and press f2.  Use the buttons
at the bottom to play the file.  If you touch a point on the chart,
data value for that point will be displayed on the right.

8) You may delete (but not rename) log files.

9) To transfer the file to a desktop/laptop system, you must have
the Tunerstein Player component installed on the p/c. 

Run the Player
Run Palm'n'Stein
Connect the Palm to the P/C using the SERIAL sync cable.  A USB Sync 
WILL NOT work!
On the Palm, press F4
Select the log file to transfer
On the P/C, click the green Palm'n'Stein button and follow the
instructions.

Please direct any questions to support@tunerstein.com
