Read the whole of this thread as the pressures are a variable due to wheel/tyre type.




2.3 => 2.3 bar where 1 bar = 15psi = 1 atmosphere

2.3 multiplied by 15 = 34.5 psi

It seems quite common for the tyres to wear excessively on the outside at the recommended pressure so the usual advice is to go 3-5 psi higher and watch the wear on the fronts. If they wear in the middle, lower the pressure and if they wear at the edges, raise the pressure.

Mine are 36 will be trying 38 shortly, as soon as I can be arsed [image: image1.png]



33 always felt too soft.

40 psi in the fronts and 38 psi in the rears seems fine on my bus, but i suppose it can be down to the rubber you use

With flitting to and fro to Germany quite often, we've found 40 psi all round works for us - lot of motorway  and constant speedo reading of 70-80 mph and a good load of stuff on board too.

36psi all round,unless i'm carrying a load [image: image2.png]


then i put 40psi in all round [image: image3.png]



40 all round here too, no problems and even wear.

38-40psi all round and have been doing for over 3 years when i first got the car the front passenger side tyre was worn on the outside when i checked the pressure it was 35psi and the others were the same so 38-40 works best for me

