If you need to change the thermostat, or just remove it for flushing the engine out you'll find it easy. These pics are from a 3CT engine (1993), later 3CT-e engines are virtually the same (except a plastic engine drain, no bleed bolt on the housing and a couple of hose clamps on the housing - obvious)
Click on the pics for bigger images:-




  
Newer type here. [image: image1.jpg]




This is the engine water drain plug. you'll need to drain the sytem to avoid water all over the engine. 

Remove the throttle cable stay bolt (12mm) [arrowed green] and push it up out of the way.Drivers side access panel removed.
Then remove the two thermostat housing bolts (10mm) [arrowed blue]. Alll a bit tight but small spanners or 1/4 inch drive socket set will fit. 
The thermostat is in a big arched alloy housing that goes over the top of the engine.



  


You must remove the bolt arrowed white to release the whole housing (from the passenger side access). 


  


wiggle the housing upwards and there is enough room to remove the thermostat.
The gasket is a rubber ring that fits around the thermostat itself. I'd recommend a new one.
Note that when replacing the thermostat there is a steel cup under it so that it only drops into place in a certain orientation.


  

Arrowed is the engine air bleed bolt. Remove this when refilling to bleed air out of the engine. (only on earlier models).


With a 3ct-e engine it can also help to take this hose off to get a bit more wiggle room to take out the thermostat.
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