hi again air lock in system driving me mad  so made a air bleed that goes in top heater core outlet details of wat and how i build it. its 3/4 inch stainless tubing made into a t. 1 off 12mm stainless steel nut and bolt welded nut to end of pipe cut 2 cuts in bolt running up the thread and 1 washer .note washer needs to be a soft metal copper,alloy.
on the tube u bolt in the  water line is a small weld to stop the hoses coming off its on the side u cant see
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