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Rear Tail Light Bulb Replacement
First of all open the tail gate........... [image: image1]
remove the 2 screws (see photo)
[image: image2]

next slide the light cluster rearwards (may take a bit of force,some use a pair of rubber gloves to grip the cluster... [image: image3])
[image: image4]

to remove the bulb simply twist the holder from the cluster
[image: image5]
[image: image6]

when bulb is replaced simply slide cluster back into place & replace screws........ [image: image7]

	

	

	

	

H4 Head Light Bulb Replacement
working from behind the light unit...........
remove the wiring connector & black plastic collar
[image: image8]

next remove the rubber seal........
[image: image9]

remove the retaining clip which holds the bulb in place.......
[image: image10]

remove bulb but make a note of the locating lugs (1,2&3) 
replace bulb & make sure it`s seated correctly in the locating lugs.......
in proper headlight alignment may result if bulb not seated correctly
[image: image11]

re-fit retaining clip,rubber seal,plastic collar & wiring connector........... [image: image12]


	

Tailgate Bulb Replacement
Remove the 4 screws/retaining clips from the tailgate trim.........
[image: image13]

gently prise the bottom edge of the trim off it`s retaining clips.......
[image: image14]
remove trim to reveal bulbs.....(these might be behind a black cover but mines missing... [image: image15])
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simply twist the bulb holder from the tailgate cluster.......
[image: image17]
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once bulb changed re-fit back into cluster & refit all trims
be carefull when replacing trim as the clips can snap easily but can be bought at most car accessory shops
[image: image19]


	

Front Fog/Aux/Driving Light Bulb Replacement
[image: image20]


with the bonnet up... [image: image21]..remove these 3 screws (might be cross-headed screws not bolts like mine)
[image: image22]
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now you can either remove the front lights completely or just leave them hanging on the wiring
to remove completely disconnect from the wiring connector.........
[image: image24]

next remove the cover to expose the bulb....
[image: image25]

remove the retaining clip holding the bulb in place & remove the bulb from the light unit...
[image: image26]

[image: image27]
disconnect the wire from the bulb & remove bulb

replacement is the reversal of the above but make sure the cut out`s on the bulb (small rectangle on one side &
semi-circle on the other) line up with the indentations in the light unit.......



	

Front Indicator Bulb Replacement
[image: image28]

I have removed the front wheel just to make it easier to take photo`s.
i believe they can be changed without removing wheel........... [image: image29]
You will have to remove the plastic wheel arch liner.............
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the liner can then be twisted out of the way.........
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if you look up inside the front wing you will see the rear of the bulb holder.......
[image: image33]
[image: image34]
as with the rear lights just twist the bulb out of it`s holder & replace.......
Re-fitting is the reversal of the above............. [image: image35]

please excuse the dirt in the photo`s......... [image: image36]


	

Front Side/Turn Lights
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first of all remove the fixing screw in the corner of the light.........
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pull light unit out at an angle from it`s aperture..........
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remove unit completely.........
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twist off bulb holder from unit.......
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remove bulb & replace......
[image: image42]

re-fitting is a reversal of the above............... [image: image43]

Note... the bulb is a 2 filament type similar to a stop/tail bulb..1 part for the side light &  the other
for the turn light(when headlights/indicators are on)



