If the over drive switch fails to work or works intermittently a very common cause is a broken wire coming from the switch on the gear lever.

If you remove the plastic cowling around the steering wheel you will see a wire coming out of the gear selector lever, the cable tends to break at the point next to the clip support. In the first 2cm or exposed cable. (it appears white in the picture below)
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For ease of repair I removed the lever (watch out for the spring it doesn't fly out but be aware)

I happened to have some twin core black flex which was soldered into place.
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Heat shrink tube would be ideal but I didn't have any that size so I used insulation tape to protect the new joins.
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The lever is then replaced (thread lock on the end of the bolt) the replaced wire was fed along the same route as the old wire. Make sure you have allowed enough slack for when the gear lever moves but more importantly for when the steering column is adjusted.
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I joined into the old wire using a screw connector.
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Test, and thats the job done, just replace the plastic cowls.

