Today I removed the engine cover and im going to show you how i have done it,


DISCLAIMERS NOTES:- IF PEOPLE WANT TO DO THE WORK, THEY DO SO AT THERE OWN RISK AND ME(JJ) NOR THE SITE TAKE NO RESPONSIBILTY FOR ANY OUT COME

Here im going to show you how i did it,
it took in total about 40mins, below i will show you in text and pictures,

First off i removed the battery leads as i going to remove the ECU later, i moved both front seats forward to leave the covers for the rear bolts and undo the 4 14mm bolts:- 
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Then you need to undo the yellow catch on both side:-



On the passager side you can now remove the seat but on the drivers side you need to undo the seatbelt warning wire and you can remove the center carpet off the engine latch:-
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Then on the drivers side undo a 10mm nut and move the switch to the petrol/diesel flap, you then need to remove the seat support there held in with 2 14mm bolts and unclip the handbrake cover (also i been informed that there is a Auxilliary amplifier there to that will have to be removed too):-
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Then on the passager side it the same but you got an extra screw as it bigger with 2 14mm bolts and it houses your ECU:-
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Here you will need to remove the plug from the ECU and put to one side then you can remove the center console you could have a box/tray or a cooler/hot box (im unsure about removing the hot/cold box as i dont have that):-
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Next is to remove the 3 10mm bolts that holds your fuse box in place as it will aid us in easier removal of the carpet:-
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So now that leave us to remove the side trims there held in with 3 screws you do this on both sides:-
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Next is what i cant show you as i dont have them on my carpet but you could have them, There are clips on the edge all you need to do is unclip them free, 

Then you need to undo the lower seat belt bolt on both sides it 14mm bolt and put to one side it helps if you knot the seat belt before you remove it ( it stops it from winding up too far ):-
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Now you can start to lift the carpet on one side you could feel a tug here and there it nothing to worry it just the velcro catching the carpet under the carpet (mouth full lol) also it helps to look around for anything that will tear the carpet so be a little gentle around the edges:-
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And then it will look like this:-
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Now you need to remove the engine latch and remove all the 12mm bolts that sit around the drivers side there are 10 bolt all together and then you can now remove the cover and put to one side (see how oily my engine is  [image: image12.png]


)
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Refitting is the reverse of the above 

Benefits= Easier to get to the engine etc,

Costs= Free,

Time= About 40min, 

Tools= 10,12,14mm socket with rachet and extension, cross head screw driver, and a straight edge screwdriver for handbrake surround,

Hope you enjoyed your tutorial and have fun ...JJ

