Start by using a small flat bladed screwdriver to remove the covers on the grab handle. 
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Unscrew the exposed screws and remove the handle. 
Gently pull away the door seal.

The door pillar trim can now be gently pulled away.
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If you need to gain extra access you can remove the small piece of trim with the air vent, using a small scraper gently lever up along its length. (there are no screws, just clips)
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And there you have it, refit in reverse order.
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Thanks Estimamike for sharing your wisdom.
