Please ignore the camera dates(knew i should of sorted that out before)
Ok,tools needed:
Small flat screwdriver
Small Philips(or star) screwdriver
Paint scraper/s or something similar.

Using the paint scrapper,gently prise of the surround  located around the heater switches.Twisting the scrapper to lift clips up.
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Next ,we need to open the doors to remove the dashboard surround.Using the flat screwdriver unclip the corners.
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Remove the two screws either side of the heater controls,then slide the flat blade screw driver along the top of the dash surround,prising out the clips.The whole unit can now be removed
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The clock assembly shoould be in full view now and ready for you to remove the 2 screws at the top and 2 either side.
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Lift out the assembly bottom first,until you can see 3 wire blocks(Brown,Blue & White) at the back of the unit,remove these.
You can now take the unit out of the van, if you so wish and proceed with removing the bulbs from the Fuel/Speedo/Rev and Temp guages to take off the green shrouds and replace.This will enable the needles to be illuminated better.
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.Now remove the clear cover by releasing the lugs around the assembly,repeat operation for the black shroud behind it.Remove the screws from the original dial face and slide the new dial over the needle,on top of the original dial.
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As my van has parking sensors i had to remove part of the face for the bus diagram to route wires behind,this is not covered in the manufacturers instructions so i had to use a bit of poetic license [image: image10.png]



The Silver surround is quite simple to fit,as all you do is remove the paper from the double sided tape and place over original surround.Replace the screws in the dial faces taking care not to overtighten,as this can damage the face.
Next drill two holes in the top of the unit for the wires to feed out wires,taking care not to damage internal workings.Reverse the process to refit all dash components.
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The unit is nearly ready to be replaced ,just the control box and power feed to take care of and we're nearly there

