Rear Tail Light Bulb Replacement
First of all open the tail gate........... 
 INCLUDEPICTURE "http://www.estimaownersclub.org/community/Smileys/classic/rolleyes.gif" \* MERGEFORMATINET 



remove the 2 screws (see photo)


next slide the light cluster rearwards (may take a bit of force,some use a pair of rubber gloves to grip the cluster... [image: image2.png]


)
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to remove the bulb simply twist the holder from the cluster
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when bulb is replaced simply slide cluster back into place & replace screws
H4 Head Light Bulb Replacement
working from behind the light unit...........
remove the wiring connector & black plastic collar
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next remove the rubber seal........
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remove the retaining clip which holds the bulb in place.......
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remove bulb but make a note of the locating lugs (1,2&3) 
replace bulb & make sure it`s seated correctly in the locating lugs.......
in proper headlight alignment may result if bulb not seated correctly
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re-fit retaining clip,rubber seal,plastic collar & wiring connector...........

Tailgate Bulb Replacement
Remove the 4 screws/retaining clips from the tailgate trim.........
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gently prise the bottom edge of the trim off it`s retaining clips.......
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remove trim to reveal bulbs.....(these might be behind a black cover but mines missing... [image: image12.png]


)
[image: image13.jpg]




simply twist the bulb holder from the tailgate cluster.......
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once bulb changed re-fit back into cluster & refit all trims
be carefull when replacing trim as the clips can snap easily but can be bought at most car accessory shops
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Front Fog/Aux/Driving Light Bulb Replacement
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with the bonnet up... [image: image18.png]


..remove these 3 screws (might be cross-headed screws not bolts like mine)
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[image: image20.jpg]




now you can either remove the front lights completely or just leave them hanging on the wiring
to remove completely disconnect from the wiring connector.........
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next remove the cover to expose the bulb....
[image: image22.jpg]




remove the retaining clip holding the bulb in place & remove the bulb from the light unit...
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[image: image24.jpg]



disconnect the wire from the bulb & remove bulb

replacement is the reversal of the above but make sure the cut out`s on the bulb (small rectangle on one side &
semi-circle on the other) line up with the indentations in the light unit.......

Front Indicator Bulb Replacement
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I have removed the front wheel just to make it easier to take photo`s.
i believe they can be changed without removing wheel........... [image: image26.png]



You will have to remove the plastic wheel arch liner.............
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 INCLUDEPICTURE "http://i16.photobucket.com/albums/b3/estimamike/32a6918d.jpg" \* MERGEFORMATINET [image: image28.jpg]



the liner can then be twisted out of the way.........
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if you look up inside the front wing you will see the rear of the bulb holder.......
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as with the rear lights just twist the bulb out of it`s holder & replace.......
Re-fitting is the reversal of the above............. [image: image32.png]




please excuse the dirt in the photo`s......... [image: image33.png]



Front Side/Turn Lights
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first of all remove the fixing screw in the corner of the light.........
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pull light unit out at an angle from it`s aperture..........
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remove unit completely.........
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twist off bulb holder from unit.......
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remove bulb & replace......
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re-fitting is a reversal of the above............... [image: image40.png]




Note... the bulb is a 2 filament type similar to a stop/tail bulb..1 part for the side light &  the other
for the turn light(when headlights/indicators are on)
