Today i removed the front bumper and im going to show you how i have done it,


DISCLAIMERS NOTES:- IF PEOPLE WANT TO DO THE WORK, THEY DO SO AT THERE OWN RISK AND ME(JJ) NOR THE SITE TAKE NO RESPONSIBILTY FOR ANY OUT COME

Here im going to show you how i did it,
it took in total about 15mins, below i will show you in text and pictures,

First you need to remove the fog lights here is the link to remove them:-
http://www.estimaownersclub.org/community/index.php?topic=22980.0

Now you need to remove the lower front wheel arch trim:-


INCLUDEPICTURE "RemoveFrontBumper/index.php_files/bits194.jpg" \* MERGEFORMAT 




There are more bolts under the bumper i forgot to take a picture sorry there are 2 bolts under the passanger side of the bumper.

And on the drivers side i had no trim there so i cant tell you what is there only an arm holding the bumper on i undone that (truth is i snapped it  )

then under each side from under the arch there are 3 screw bolts holding the bumper to the wing I could not get a picture as it was a tight area to get the camera in :-
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Then there are 6 bolts holding in the front 4 on the inside you will see it next to the headlight under the removed foglights:-

Driver side:-
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Passanger side:-
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Then there 2 bolts outside at the lower end of the bumper :-
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Now you can move the bumper out but as you pull it out there are 2 wires holding the sidelights in just undo them :-
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And this what it will look like with the bumper removed:-
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to refit it just reverse the above

Benefits= to replace or get your head light out or get to your intercooler,

Costs= Free 

Time= About 15min 

Tools= 10,12,14mm socket with extension and ratchet,

Hope you enjoyed your tutorial and have fun ...JJ

