Hello all

After reading all the horror stories i've just done my front shocks. Not too bad really, but i wouldn't atempt it without certain items of kit, i've made a list.

1. a selection of 3/8 drive[1/2 in are too bulky]  rachets or pull bars, 14mm rachet and ring spanners.The top bolts on the drivers side needed a long 3/8 bar and 14mm socket to shift them then a rachet spanner or ring spanner to get off.

2. 22mm socket and spanner with long pull bar. the bottom bolts are big 22mm jobs just need a big pull, remember to turn the nut not the bolt.

3. long allen keys or allan 'bits' The antiroll bar tie rods have an iternal allen fitting and a 17mm outer so you need both, else the bolt just goes round as you try to undo the nut.

4. brake hose clamps. you need to remove the short solid pipe from the strut and clamp the flexi.

5. good long spring compressors. my mate did this bit for me and he used 4 mole grips tp help  stop the compressors sliding off to the side.

it really wasn't too bad just get the right gear together first and remember to bleed the brakes afterwards!!

gareth
